Application Setting Page

General Settings
Number of Motors Single motor Dual motor Triple motor | Motor Types Motor #1 : Motor #2 : Motor #3 : | Data Type Representation 16-bit fixed-point 32-bit fixed-point 32-bit floating-point | Discretization Method
IIRx Filter Coef Scale Divided by:
Project Path Selection
| Project path: C://
Motor Selection to be set |  |
MCAT Tab Manager
| Position/Speed Settings Position/Speed Sensors Encoder Resolver Sensorless Hall Sincos | Position/Speed ATO Parallel TO PI Recurrent TO PI Speed Feedback Filter | BEMF DQ Observer Parallel PI Recurrent PI Position/Speed sensors Encoder Resolver Sensorless Hall Sincos | Position/Speed ATO Parallel TO PI Recurrent TO PI Speed Feedback Filter: | BEMF DQ Observer Parallel PI Recurrent PI Position/Speed Sensors Encoder Resolver Sensorless Hall Sincos | Position/Speed ATO Parallel TO PI Recurrent TO PI Speed Feedback Filter: | BEMF DQ Observer Parallel PI Recurrent PI
Control Loop Settings Current Control Loop Parallel Current PI Recurrent Current PI Feedforward path: | Speed Control Loop Parallel Speed PI Recurrent Speed PI Feedforward path: | Zero Position Alignment Align Voltage Align Current Current Control Loop Parallel Current PI Recurrent Current PI Feedforward path: | Speed Control Loop Parallel Speed PI Recurrent Speed PI Feedforward path: | Zero Position Alignment Align Voltage Align Current Current Control Loop Parallel Current PI Recurrent Current PI Feedforward path: | Speed Control Loop Parallel Speed PI Recurrent Speed PI Feedforward path: | Zero Position Alignment Align Voltage Align Current