- ### Webserver Home

- ### Network Status...

  - IP Stats
  - ICMP Stats
  - UDP Stats
  - TCP Stats
- System Run Time (RTC)
- LED Control

- ### Configuration Pages

  - LTC2600 DAC
  - LTC2704 DAC
  - LTC2498 ADC
  - LTC1859 ADC
- ADC Datalogger Config
- Thermocouple Reader

# Multi-Channel ADC Datalogger Configuration Page

This is the page to configure the LTC 1859 and LTC 2498 ADCs for data logging

The system will sample all the selected channels every [sampleinterval] milliseconds.
ADCs that are too slow to maintain the sampling rate will wait until the next sample clock tick.
The system will stop after [numsamples] samples have been taken per (fastest) channel.
This data will be written to a .csv file with name [logfilename] on the USB flash drive.

There is also the ability to write to the DACs after each round of samples using the Data File.

How to write the Data File: Data File Example

## Sampling Interval (ms):
Number of Samples (per channel):
Read from Datafile to DACs:
Enabled
1859 Channel Setting:
Differential 0:1
Differential 2:3
Differential 4:5
Differential 6:7
Differential 1:0
Differential 3:2
Differential 5:4
Differential 7:6
Single-Ended 0
Single-Ended 1
Single-Ended 2
Single-Ended 3
Single-Ended 4
Single-Ended 5
Single-Ended 6
Single-Ended 7
Span Setting:
Bipolar [-5V to 5V]
Bipolar [-10V to 10V]
Unipolar [0 to 5V]
Unipolar [0 to 10V]

# Datalogger State:

## Sampling...

## Logfile Name (without .csv suffix):
Datafile Name (without .csv suffix):
2498 Channel Setting:
Differential 0:1
Differential 2:3
Differential 4:5
Differential 6:7
Differential 1:0
Differential 3:2
Differential 5:4
Differential 7:6
Single-Ended 0
Single-Ended 1
Single-Ended 2
Single-Ended 3
Single-Ended 4
Single-Ended 5
Single-Ended 6
Single-Ended 7
External Input - Speed and Rejection Setting:
Reject 50/60 Hz, x1 speed
Reject 50 Hz, x1 speed
Reject 60 Hz, x1 speed
Reject 50/60 Hz, x2 speed
Reject 50 Hz, x2 speed
Temperature Sensor - Speed and Rejection Setting:
Reject 50/60 Hz, x1 speed
Reject 50 Hz, x1 speed
Reject 60 Hz, x1 speed

© Freescale Semiconductor, Inc. 2004 - 2008. All Rights Reserved
© Linear Technology Corporation. 1981 - 2010. All Rights Reserved