- ### Webserver Home

- ### Network Status...

  - IP Stats
  - ICMP Stats
  - UDP Stats
  - TCP Stats
- System Run Time (RTC)

- ### Configuration Pages

  - LTC2600 DAC
  - LTC2704 DAC
  - LTC2498 ADC
  - LTC1859 ADC
- ADC Datalogger Config
- Thermocouple Reader

# LTC 2704 Configuration Page

This is the page to configure the LTC 2704 4-channel 16-bit SoftSpan Digital to Analog Converter

Datasheet: LTC2704 - 4ch 16bit SoftSpan DAC

## Value to Write: Vref:
Channel Setting:
Span Setting:
Unipolar [0 to 5V]
Unipolar [0 to 10V]
Bipolar [-5V to 5V]
Bipolar [-10V to 10V]
Bipolar [-2.5V to 2.5V]
Bipolar [-2.5V to 7.5V]
Command Setting - Write and Update:
Write Code/Span N
Write Code/Span N and Update N
Write Code/Span N and Update All
Update N
Update All

Value to Write:

## Command Setting - Read:
Read B1 Span N
Read B1 Code (Value) N
Read B2 Span N
Read B2 Code (Value) N
Command Setting - Sleep:
Sleep
No Operation

© Freescale Semiconductor, Inc. 2004 - 2008. All Rights Reserved
© Linear Technology Corporation. 1981 - 2010. All Rights Reserved