MM912H634 Ctrl Panel |  |
Last Error Message: |
Status
Last reset: | WDR | EXR | WUR | LVRX | LVR | POR
| Last wake-up event: | FWU | LINWU | L5WU | L4WU | L3WU | L2WU | L1WU | L0WU
Voltage monitor: | HTC | HVC | LVC | LBC

Enable Watch dog |

LIN

| Enable LIN
| Baud rate: | 19 200 | Size of the message: | 4 bytes |
| LIN slave ID : | 0x10 | LIN Received Message: |

Switches Control and Pulse Width Modulation

Enable PWM Channel 0
Enable PWM Channel 1
Channel 0 Setting Channel 1 Setting

| Positive
Negative

HS1 PWM Enable Source CH0
Source CH1
HS2 PWM Enable Source CH0
Source CH1
LS1 PWM Enable Source CH0
Source CH1
LS2 PWM Enable Source CH0
Source CH1
PTB2 PWM Enable Source CH0
Source CH1
Analog Inputs

Battery voltage: |  | V
Temperature: |  | °C
Load current: |  | raw
Lx Visualization

L0
L1
| L2 --- | L3 | L4 | L5 | Range 5 V
Range 18 V

AD0 ---
AD1 ---
| AD2 ---

Wake up

Lx
Forced
None

L0 | L1 | L2 |
Cyclic Sense |  | HS1 HS2
L3 | L4 | L5 |

Basic Timer | Multiplier |  |